**Monitor**Screen: 5-inch IPS HD Display  
Screen Resolution: 854x480 pixels (FWVGA)  
Image Capturing Resolution: 1920x1080 pixels (JPG)  
Video Recording Resolution: 1280x720 pixels (MOV)  
Port: Micro USB charging port / Micro SD card slot  
Storage: 32GB Micro SD card  
Flash Light: 1 Watt Cree LED  
Power Source: 5000mAh lithium battery  
Battery Life: 5-6 hours  
Operating Temperature: 32° to 113°F (0° to 45°C)

**Camera**Type: Dual Lens, Straight-viewing and Side-viewing  
Diameter: 0.21 in (5.5 mm) / 0.31 in (8.0 mm)  
Probe Length: 3.2 ft (1-meter) / 9.8 ft (3-meters) / 16 ft (5-meters)  
Probe Stiffness: Medium / Stiff  
Megapixel: 2.0 Megapixel  
Resolution: 1280x720 pixels  
Viewing Angle: 70º  
Depth of Field:   
     Straight-viewing Camera: 1.18 in to 3.15 in (30 mm to 80 mm)  
     Side-viewing Camera: 0.79 in to 1.97 in (20 mm to 50 mm)  
LED Light: 6 Adjustable High-intensity LEDs  
Splash, Water, and Dust Resistant: Rated IP67 (maximum depth of 1 meter up to 30 minutes) under IEC standard 60529